**Coomera to Helensvale Duplication**

Night works – Coomera rail corridor

December 2016

Queensland Rail is duplicating the final section of single track on the Gold Coast line, between Coomera and Helensvale stations. The Coomera to Helensvale Duplication involves construction of 8.2 kilometres of track and eight rail bridges, installing overhead electrification and signalling systems, and replacing 3.8 kilometres of timber barrier fencing.

**On Monday 19 and Tuesday 20 December 2016, night works will be undertaken in the rail corridor between Foxwell Road and the Coomera River in Coomera. These works will occur between 11pm and 5am each night, weather permitting.**

Project workers will be unloading heavy rails from rail trains and placing them in formation along the corridor in preparation for track works. These works must be undertaken at night to minimise any disruption to train services.

**Overview of work**

|  |  |  |
| --- | --- | --- |
| **Location** | **Dates and hours of night works** | **Type of work** |
| Rail corridor between Foxwell Road and Coomera River | **Between 11pm and 5am on the following nights:*** **Monday 19 December**
* **Tuesday 20 December**
 | * Rail traffic in the corridor overnight
* Unloading of new rails from rail train
* Use of heavy equipment, machinery and vehicles to move rails from the rail train into formation on the rail line
* Use of mobile lighting towers
* Access to rail corridor by project workers, vehicles and machinery.
 |
| Residents and businesses located near this area may experience increased night time noise from the presence of trains in the corridor and rails being unloaded from rail trains. Residents may also be impacted by the use of lighting associated with this activity.Queensland Rail apologises for any inconvenience and appreciates the local community’s cooperation during these important works.  |

For more information about this project please phone **1800 664 484** (during construction hours), email **C2H@qr.com.au** or visit **queenslandrail.com.au/C2H**